{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"external_links":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":32,"n_cols":2,"rows_kept":32,"merged":[[1,0,1,1],[5,0,7,0],[8,0,10,0],[12,0,14,0],[20,0,24,0],[25,0,28,0],[29,0,30,0]],"flags":["formulas_cached_only"]}
["附件1"]
["2014年工业行业淘汰落后和过剩产能中央财政奖励门槛"]
["行业","奖励门槛"]
["炼铁","400立方米及以上高炉"]
["炼钢","30吨及以上转炉、电炉"]
["焦炭","炭化室4.3米（捣固焦炉3.8米）及以上常规焦炉"]
[null,"单炉产能7.5万吨/年及以上兰炭炭化炉"]
[null,"产能40万吨及以上的热回收焦炉"]
["铁合金","6300千伏安及以上铁合金矿热电炉"]
[null,"1500千伏安及以上铁合金硅钙合金电炉和硅钙钡铝合金电炉"]
[null,"电解金属锰5000千伏安以上的整流变压器生产线"]
["电石","单台变压器容量12500千伏安及以上电石炉"]
["造纸","单条年生产能力3.4万吨及以上的非木浆生产线"]
[null,"单条年生产能力1.7万吨及以上的化学木浆生产线"]
[null,"单条年生产能力1万吨及以上以废纸为原料的制浆生产线"]
["水泥","窑径3米及以上的机械化立窑熟料生产线、窑径2.5米及以上的干法中空窑熟料生产线、干法旋窑熟料生产线"]
["平板玻璃","60万重量箱及以上平拉（含格法）生产线"]
["电解铝","100千安及以上预焙槽"]
["铜冶炼","密闭鼓风炉、反射炉、电炉炼铜工艺及设备"]
["铅冶炼","已配套建设制酸及尾气吸收系统的烧结机炼铅工艺及设备"]
["印染","前处理生产线"]
[null,"后整理生产线（包括拉幅、定形设备）"]
[null,"印花生产线（包括圆网或平网印花机）"]
[null,"连续染色生产线"]
[null,"间歇式染色机"]
["化纤","1万吨/年及以上粘胶短纤生产线"]
[null,"DMF溶剂法腈纶生产线"]
[null,"采用锭轴长900mm以下半自动卷绕设备的涤纶长丝生产线"]
[null,"3万吨/年及以上间歇法聚酯聚合生产线"]
["制革","年加工生皮能力3万标张牛皮及以上的生产线"]
[null,"年加工蓝湿皮能力3万标张牛皮及以上的生产线"]
["铅蓄电池","所有铅蓄电池生产线"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}